**Electricity Supply Request**

Please list **each and every item** of electrical equipment you propose to connect to the festival's power supply and specify the loading and supply requirement for each item (including supplies for specific equipment, kettles, lighting, etc). Failure to provide the required information may result in your supply being restricted.

**The IEE Regulations require that a 16A connection is the only acceptable means of connecting to a CBC external power supply. 13A connections alone, or by use of a 13A / 16A adapter are not acceptable and will not be connected to a festival power supply. The festival will provide a 16A mains supply cable to your stall with a “female” socket. It is your responsibility to provide a 16A “male” socket in order to connect to this supply. It is a requirement that cable used by you shall be less than 2.5mm2 duty cable.**

* 16A supplies are available; however, these are not to be exceeded in one single feed from the mains supply
* 32A supplies are available in specific locations; however these are very limited, and are not to be exceeded
* 1 item of electrical equipment will require one 16A connection and feed. More than 1 items of equipment to be connected must be supplied by a 16A multi-gang. You are solely responsible for all wiring and equipment
* All electrical equipment to be used by the trader must display a current and valid Portable Appliance Test Certificate
* No connection will be made to the festival's mains power supply unless the inspecting electrician is

satisfied the above requirements have been met

**I require an electricity supply:** **YES / NO**

|  |  |
| --- | --- |
| **Item Description** | **Electrical loading of proposed equipment** |
| 1 | Kw |
| 2 | Kw |
| 3 | Kw |
| 4 | Kw |
| 5 | Kw |
| **TOTAL LOAD REQUIRED** | **Kw** |